Minimum equipment list for delivery of Light Vehicle/Motor Cycle MOT training

* Vehicle Ramp with Turning Plates & Jacking Beam or:-
* Vehicle Pit with Jacking Beam
* Roller Brake Tester
* Headlamp Aim Tester
* Gas Analyser\*
* Diesel Smoke Meter\*
* Corrosion Assessment Tool (CAT)
* Tyre Tread Depth Gauge
* Decelerometer
* Low voltage hand lamp
* Steel tape (Minimum 1 metre)
* 13 Pin trailer socket tester
* Gas leak detector (Optional – only required for gas vehicles)

Motorcycle

* Brake Tester with Weighing Facility or:-
* Brake Tester incorporating Weighing Facility
* Headlamp Aim Tester
* Corrosion Assessment Tool (CAT)
* Tyre Tread Depth Gauge
* Decelerometer
* Selection of levers
* Low voltage hand lamp
* Steel tape (Minimum 1 metre)
* Wheel alignment cords or bars

*\*Equipment should be as currently authorised for MOT use but need not be calibrated*